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Ethyl acetate

According to Regulation (EU) 2020/878 (REACH Annex II) · CLP (EC) 1272/2008 as amended by EU 2024/2865
SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1 Product identifier
	Property
	Value

	Product form
	Substance

	Chemical name
	Ethyl acetate

	EC Index-No.
	607-022-00-5

	EC-No.
	205-500-4

	CAS-No.
	141-78-6

	REACH registration No.
	01-2119475103-46-XXXX

	Molecular formula
	C₄H₈O₂


1.3 Details of the supplier of the safety data sheet
	Field
	Details

	Company
	Synthesia Ltd.

	Address
	Todor Radunchev 9, Krivina 1588, Bulgaria

	VAT
	BG121306542

	Phone
	+359 2 974 4968

	Email
	office@synthesia.bg


1.4 Emergency telephone number
Emergency number: 112
SECTION 2: Hazards identification
2.1 Classification of the substance or mixture
	Hazard class
	Category
	Hazard statement

	Flammable liquids
	Category 2
	H225 — Highly flammable liquid and vapour

	Serious eye damage/eye irritation
	Category 2
	H319 — Causes serious eye irritation

	STOT — Single exposure
	Category 3 (Narcosis)
	H336 — May cause drowsiness or dizziness


2.2 Label elements
	Element
	Details

	Hazard pictograms
	GHS02 (Flame) · GHS07 (Exclamation mark)

	Signal word
	DANGER

	Hazard statements
	H225 — Highly flammable liquid and vapour.
H319 — Causes serious eye irritation.
H336 — May cause drowsiness or dizziness.

	EUH-statements
	EUH066 — Repeated exposure may cause skin dryness or cracking.


2.3 Other hazards
This substance does not contain components considered to be PBT, vPvB, PMT, or vPvM at levels of 0.1% or higher, in accordance with CLP regulation as amended by EU 2024/2865 and REACH Annex XIII.
Not classified as an endocrine disruptor (ED) according to CLP 2024/2865, Commission Delegated Regulation (EU) 2017/2100, or Commission Regulation (EU) 2018/605.
Vapours may form explosive mixture with air.
SECTION 3: Composition/information on ingredients
3.1 Substances
	Component
	CAS-No.
	EC-No.
	Index-No.
	Classification
	Conc.

	Ethyl acetate
	141-78-6
	205-500-4
	607-022-00-5
	Flam. Liq. 2; Eye Irrit. 2; STOT SE 3
	> 99.8%


Molecular weight: 88.11 g/mol | Formula: C₄H₈O₂
3.2 Mixtures: Not applicable.
SECTION 4: First aid measures
	Route
	Measures

	Inhalation
	Remove person to fresh air and keep comfortable for breathing.

	Skin contact
	Rinse skin with water/shower. Remove contaminated clothing.

	Eye contact
	Rinse cautiously with water for several minutes. Remove contact lenses.

	Ingestion
	Rinse mouth. Do not induce vomiting. Call a poison centre.


SECTION 5: Firefighting measures
Suitable extinguishing media: Water spray, dry powder, foam, CO₂.
Unsuitable: High volume water jet.
Special hazards: Highly flammable liquid and vapour. Toxic fumes (carbon oxides).
SECTION 6: Accidental release measures
Personal precautions: Wear PPE. Ventilate area. No open flames. Avoid vapours.
Environmental precautions: Avoid release to the environment.
Containment: Take up with absorbent material. Notify authorities if entering sewers/waters.
SECTION 7: Handling and storage
Keep away from heat, sparks, open flames. Ground/bond container. Use non-sparking tools. Explosion-proof equipment.
Storage: Well-ventilated place. Keep cool. Keep container tightly closed. Store locked up.
SECTION 8: Exposure controls/personal protection
OEL TWA: 734 mg/m³ (200 ppm) | OEL STEL: 1,468 mg/m³ (400 ppm) | Ref: Directive (EU) 2017/164 · SCOEL 2008
PPE: Gloves, safety glasses, protective clothing. Respiratory protection if ventilation insufficient.
SECTION 9: Physical and chemical properties
	Property
	Value

	Physical state
	Liquid

	Appearance
	Colourless, clear

	Odour
	Fruity

	Melting point
	-84 °C

	Boiling range
	76.5 – 77.5 °C

	Flash point
	-4 °C

	Auto-ignition
	426 °C

	Flammability limits
	2 – 11.5 vol %

	Vapour pressure
	73 mm Hg (20 °C)

	Density
	0.902 g/cm³ (20 °C)

	Solubility (water)
	8 g/100 ml (25 °C)

	log Pow
	0.73

	Viscosity
	0.45 mPa·s (20 °C)


SECTION 10: Stability and reactivity
Reactivity: Highly flammable liquid and vapour.
Stability: Stable under normal conditions.
Conditions to avoid: Heat, open flames, sparks, ignition sources.
SECTION 11: Toxicological information
Acute toxicity: Not classified.
LD50 oral (rabbit): 5,620 mg/kg bw (rabbit)
LD50 dermal (rat): > 18,000 mg/kg bw (rat)
LC50 inhalation (rat): 1.600 mg/l/4h (rat)
Eye irritation: Category 2 — Causes serious eye irritation.
STOT SE: Category 3 — May cause drowsiness or dizziness.
Repeated dose: NOAEL 900 mg/kg bw, LOAEL 3,600 mg/kg bw (oral, rat, 90d)
Endocrine disrupting properties: Not classified per CLP 2024/2865, Reg. 2017/2100, or Reg. 2018/605.
SECTION 12: Ecological information
Fish LC50 (96h): 230 mg/l (Pimephales promelas)
Daphnia EC50 (48h): 720 mg/l (Daphnia magna)
Biodegradation: 100 % — 28 days — Readily biodegradable
Log Pow: 0.73 — low bioaccumulation potential
Not PBT or vPvB per REACH Annex XIII.
SECTION 13: Disposal considerations
Dispose in accordance with local/national/international regulations.
Do not re-use empty containers. Flammable vapours may accumulate.
SECTION 14: Transport information
	Mode
	UN No.
	Shipping name
	Class
	PG

	ADR (road)
	1173
	ETHYL ACETATE
	3
	II

	IMDG (sea)
	1173
	ETHYL ACETATE
	3
	II

	IATA (air)
	1173
	Ethyl acetate
	3
	II

	ADN (inland)
	1173
	ETHYL ACETATE
	3
	II

	RID (rail)
	1173
	ETHYL ACETATE
	3
	II


Tunnel code: D/E | Kemler: 33 | Transport cat: 2
Limited qty: 1 L | Excepted qty: E2
SECTION 15: Regulatory information
REACH Annex XVII: No restrictions. Not on SVHC Candidate List or Annex XIV.
PIC Reg. (EU) 649/2012: Not subject. POP Reg. (EU) 2019/1021: Not subject.
Germany WGK: WGK 1 — Slightly hazardous to water (AwSV; ID No. 95)
Denmark: Young persons under 18 not allowed to use the product.
SECTION 16: Other information
	Code
	Text

	H225
	Highly flammable liquid and vapour.

	H319
	Causes serious eye irritation.

	H336
	May cause drowsiness or dizziness.

	EUH066
	Repeated exposure may cause skin dryness or cracking.


Abbreviations: ADN, ADR, CAS, CLP, DMEL, DNEL, EC50, ED, IATA, IMDG, LC50, LD50, LOAEL, NOAEL, PBT, PMT, PNEC, REACH, RID, SDS, STOT, vPvB, vPvM, WGK

Disclaimer of Liability: The information in this SDS was obtained from sources which we believe are reliable. However, the information is provided without any warranty, express or implied, regarding its correctness. The conditions or methods of handling, storage, use or disposal of the product are beyond our control and may be beyond our knowledge.
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