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SAFETY DATA SHEET
Ethyl acetate

According to Regulation (EU) 2020/878 (REACH Annex II) · CLP (EC) 1272/2008 as amended by EU 2024/2865
  SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1 Product identifier
	Property
	Value

	Product form
	Substance

	Chemical name
	Ethyl acetate

	EC Index-No.
	607-022-00-5

	EC-No.
	205-500-4

	CAS-No.
	141-78-6

	REACH registration No.
	01-2119475103-46-XXXX

	Molecular formula
	C₄H₈O₂


1.2 Relevant identified uses and uses advised against
Use of the substance/mixture: Industrial use
Restrictions on use: No data available
1.3 Details of the supplier of the safety data sheet
	Field
	Details

	Company
	Synthesia Ltd.

	Address
	Todor Radunchev 9, Krivina 1588, Bulgaria

	VAT
	BG121306542

	Phone
	+359 2 974 4968

	Email
	office@synthesia.bg


1.4 Emergency telephone number
Emergency number: 112
  SECTION 2: Hazards identification
2.1 Classification of the substance or mixture
Classification according to Regulation (EC) No. 1272/2008 [CLP] as amended by EU 2024/2865:
	Hazard class
	Category
	Hazard statement

	Flammable liquids
	Category 2
	H225 — Highly flammable liquid and vapour

	Serious eye damage/eye irritation
	Category 2
	H319 — Causes serious eye irritation

	Specific target organ toxicity — Single exposure
	Category 3 (Narcosis)
	H336 — May cause drowsiness or dizziness


Full text of H-statements: see Section 16.
2.2 Label elements
	Element
	Details

	Hazard pictograms
	GHS02 (Flame) · GHS07 (Exclamation mark)

	Signal word
	DANGER

	Hazard statements
	H225 — Highly flammable liquid and vapour.
H319 — Causes serious eye irritation.
H336 — May cause drowsiness or dizziness.

	Precautionary statements
	P210 — Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.
P280 — Wear protective gloves/protective clothing/eye protection/face protection.
P304+P340 — IF INHALED: Remove person to fresh air and keep comfortable for breathing.
P305+P351+P338 — IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.
P337+P313 — If eye irritation persists: Get medical advice/attention.
P403+P233 — Store in a well-ventilated place. Keep container tightly closed.

	EUH-statements
	EUH066 — Repeated exposure may cause skin dryness or cracking.


2.3 Other hazards
This substance does not contain components considered to be PBT, vPvB, PMT, or vPvM at levels of 0.1% or higher, in accordance with the criteria of CLP Regulation as amended by EU 2024/2865 and REACH Annex XIII.
Not classified as an endocrine disruptor (ED) according to CLP 2024/2865, Commission Delegated Regulation (EU) 2017/2100, or Commission Regulation (EU) 2018/605.
Vapours may form explosive mixture with air.
  SECTION 3: Composition/information on ingredients
3.1 Substances
	Component
	CAS-No.
	EC-No.
	Index-No.
	Classification
	Conc.

	Ethyl acetate
	141-78-6
	205-500-4
	607-022-00-5
	Flam. Liq. 2; Eye Irrit. 2; STOT SE 3
	> 99.8%


Molecular weight: 88.11 g/mol | Formula: C₄H₈O₂
3.2 Mixtures: Not applicable.
  SECTION 4: First aid measures
4.1 Description of first aid measures
	Route
	Measures

	General
	Call a poison centre or a doctor if you feel unwell.

	Inhalation
	Remove person to fresh air and keep comfortable for breathing.

	Skin contact
	Rinse skin with water/shower. Remove contaminated clothing.

	Eye contact
	Rinse cautiously with water for several minutes. Remove contact lenses. Continue rinsing. If irritation persists: Get medical advice.

	Ingestion
	Rinse mouth. Do not induce vomiting. Call a poison centre or a doctor if you feel unwell.


4.2 Most important symptoms and effects
May cause drowsiness or dizziness. Repeated exposure may cause skin dryness or cracking. Causes eye irritation.
4.3 Indication of immediate medical attention
Treat symptomatically.
  SECTION 5: Firefighting measures
5.1 Extinguishing media
Suitable: Water spray, dry powder, foam, CO₂.
Unsuitable: High volume water jet.
5.2 Special hazards
Highly flammable liquid and vapour. Toxic fumes may be released (carbon oxides).
5.3 Advice for firefighters
Self-contained breathing apparatus. Complete protective clothing.
  SECTION 6: Accidental release measures
6.1 Personal precautions
Wear PPE. Ventilate area. No open flames. Avoid breathing vapours.
For emergency responders: Eliminate ignition sources. Evacuate unnecessary personnel.
6.2 Environmental precautions
Avoid release to the environment.
6.3 Containment and cleaning up
Take up with absorbent material. Notify authorities if product enters sewers or public waters.
  SECTION 7: Handling and storage
7.1 Precautions for safe handling
Keep away from heat, sparks, open flames. Ground/bond container. Use non-sparking tools. Explosion-proof equipment. Avoid breathing vapours.
7.2 Conditions for safe storage
Store in well-ventilated place. Keep cool. Keep container tightly closed. Store locked up.
  SECTION 8: Exposure controls/personal protection
8.1 Control parameters
IOELV TWA: 734 mg/m³ (200 ppm)
IOELV STEL: 1,468 mg/m³ (400 ppm)
8.2 Exposure controls
Engineering: Good ventilation.
PPE: Gloves, safety glasses, protective clothing.
Respiratory: If insufficient ventilation.
  SECTION 9: Physical and chemical properties
Appearance
Clear, colourless liquid
Odour
Fruity
Melting point
-84 °C
Boiling point
76.5 – 77.5 °C
Flash point
-4 °C
Auto-ignition temp.
426 °C
Vapour pressure
73 mm Hg (20 °C)
Density
0.902 g/cm³ (20 °C)
Solubility in water
8 g/100 ml (25 °C)
log Pow
0.73
Flammability limits
2 – 11.5 vol %
  SECTION 10: Stability and reactivity
10.1 Reactivity
Highly flammable liquid and vapour.
10.2 Chemical stability
Stable under normal conditions.
10.4 Conditions to avoid
Heat, open flames, sparks, ignition sources.
  SECTION 11: Toxicological information
Acute toxicity
Not classified. LD50 oral: 5,620 mg/kg. LC50 inhalation: 1.600 mg/l/4h.
Eye irritation
Causes serious eye irritation.
STOT single exposure
Category 3 — May cause drowsiness or dizziness.
  SECTION 12: Ecological information
12.1 Toxicity
Not harmful to aquatic organisms.
LC50 (fish, 96h): 230 mg/l
EC50 (daphnia, 48h): 720 mg/l
12.2 Persistence
Readily biodegradable — 100% after 28 days.
12.3 Bioaccumulation
Log Pow 0.73 — low bioaccumulation potential.
  SECTION 13: Disposal considerations
13.1 Waste treatment
Dispose in accordance with local/national/international regulation.
Do not re-use empty containers.
  SECTION 14: Transport information
UN number
1173
Proper shipping name
ETHYL ACETATE
Class
3
Packing group
II
ADR tunnel code
D/E
IMDG EmS
F-E, S-D
  SECTION 15: Regulatory information
REACH Annex XVII
No restrictions
SVHC Candidate List
Not listed
Annex XIV (Authorisation)
Not listed
Germany WGK
WGK 1 — Slightly hazardous to water
  SECTION 16: Other information
H225
Highly flammable liquid and vapour.
H319
Causes serious eye irritation.
H336
May cause drowsiness or dizziness.
EUH066
Repeated exposure may cause skin dryness or cracking.

Disclaimer of Liability:
The information in this SDS was obtained from sources which we believe are reliable. However, the information is provided without any warranty, express or implied, regarding its correctness. The conditions or methods of handling, storage, use or disposal of the product are beyond our control and may be beyond our knowledge. For this and other reasons, we do not assume responsibility and expressly disclaim liability for loss, damage or expense arising out of or in any way connected with the handling, storage, use or disposal of the product.
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